wfb

wfh-

wfhl+

wfr-

wfrl+

wfve+

v

x

uf

mode

ph

pl

pr

per

fexth

fextr

xol

ACTUATOR\_A\_B