wfs-

wfd­­­+

wfh-

wfvrs-wfvr+

wfvx+

v

x

uf

mode

ps

pd

ph

prs

pr

pxr

xol

VALVE\_A